{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["设计构想"],"not_rendered":{"images":3,"external_links":1,"defined_names":11},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"设计构想","index":0,"n_rows":54,"n_cols":26,"rows_kept":54,"merged":[[1,1,4,3],[1,4,4,23],[5,1,6,3],[5,4,6,9],[5,10,6,21],[5,22,6,25],[7,1,16,3],[7,4,7,9],[7,10,7,21],[7,22,7,25],[8,4,8,9],[8,10,8,21],[8,22,8,25],[9,4,9,9],[9,10,9,21],[9,22,9,25],[10,4,10,9],[10,10,10,21],[10,22,10,25],[11,4,11,9],[11,10,11,21],[12,4,12,9],[12,10,12,21],[12,22,12,25],[13,4,13,9],[13,10,13,21],[13,22,13,25],[14,4,14,9],[14,10,14,21],[14,22,14,25],[15,4,15,9],[15,10,15,21],[15,22,15,25],[16,4,16,9],[16,10,16,21],[16,22,16,25],[17,1,18,9],[17,10,17,21],[17,22,17,25],[18,10,18,21],[18,22,18,25],[19,1,19,9],[19,10,19,21],[19,22,19,25],[20,1,20,9],[20,10,20,21],[20,22,20,25],[21,1,21,9],[21,10,21,21],[21,22,21,25],[22,1,22,7],[22,10,22,21],[23,1,23,7],[23,10,23,21],[24,1,24,9],[24,10,24,21],[24,22,24,25],[25,1,25,9],[25,10,25,21],[25,22,25,25],[26,1,26,9],[26,10,26,21],[26,22,26,25],[27,1,27,9],[27,10,27,21],[27,22,27,25],[28,1,28,9],[28,10,28,21],[28,22,28,25],[29,1,29,9],[29,10,29,21],[29,22,29,25],[30,1,30,9],[30,10,30,21],[30,22,30,25],[31,1,31,9],[31,10,31,21],[31,22,31,25],[32,1,32,9],[32,10,32,21],[32,22,32,25],[33,1,33,9],[33,10,33,21],[33,22,33,25],[34,1,34,9],[34,10,34,21],[34,22,34,25],[35,1,36,9],[35,10,35,21],[35,22,36,25],[36,10,36,21],[37,1,37,9],[37,10,37,21],[37,22,37,25],[38,1,38,9],[38,10,38,21],[38,22,38,25],[39,1,39,9],[39,10,39,21],[39,22,39,25],[40,1,40,9],[40,10,40,21],[40,22,40,25],[41,1,41,9],[41,10,41,21],[41,22,41,25],[42,1,42,9],[42,10,42,21],[42,22,42,25],[43,1,43,9],[43,10,43,21],[43,22,44,25],[44,1,44,9],[44,10,44,21],[45,1,45,9],[45,10,45,21],[45,22,45,25],[46,1,46,9],[46,10,46,21],[46,22,46,25],[47,1,47,9],[47,10,47,21],[47,22,47,25],[48,1,48,3],[48,4,48,6],[48,7,48,9],[48,10,48,21],[48,22,48,25],[49,1,50,3],[49,4,50,6],[49,7,50,9],[49,10,49,21],[50,10,50,21],[50,22,50,25]],"flags":["formulas_cached_only"]}
[null,"　"]
[{"$nulls":4},"K10前保险杠下格栅设计构想书",{"$nulls":19},"页    号","共 2 页  第 1 页"]
[{"$nulls":24},"项目名称","K10"]
[{"$nulls":24},"版   本","A01"]
[{"$nulls":24},"文件编号"]
[null,"项目",null,null,"开发目标/特性",{"$nulls":5},"技术要求、设计目标及基本结构",{"$nulls":11},"主要试验项目"]
[]
[null,"K10",{"$nulls":8},"1、设计目标\n  ",{"$nulls":11},"XMQT 018《模制塑料件(外饰零件)的试验方法》"]
[{"$nulls":10}," 1) 保护功能：在汽车发生纵向碰撞时，能吸收部分能量，以保护车身。",{"$nulls":11},"GB / T 9286-1998《 色漆和清漆漆膜的划格试验》"]
[{"$nulls":10}," 2) 装置功能：在前保险杠上安装灯具、牌照、装饰件等器件。"]
[{"$nulls":10}," 3) 美化功能"]
[{"$nulls":10},"2、技术要求"]
[{"$nulls":10}," 1) 外观要求：表面应平整，轮廓清晰，线条柔和，无缩痕、无银丝、无裂纹、无明显熔接痕。"]
[{"$nulls":10}," 2)格栅应符合GB 20182—2024《商用车驾驶室外部凸出物》等相关规定和标准。\n"]
[{"$nulls":10}," 3) 总成中的零部件应满足以下要求，并提供相关PPAP资料："]
[{"$nulls":10},"a、耐热循环性、耐加速自然老化性、耐振动性、耐水性、耐化学性、耐冲击性等应满足XMQT 018《模制塑料件(外饰"]
[{"$nulls":10},"零件)的试验方法》的相关规定和标准"]
[null,"法规要求",{"$nulls":8},"b、附着力应满足GB/T 9286-1998《色漆和清漆漆膜的划格试验》标准要求；试验结果不低于2级；"]
[{"$nulls":10},"c、格栅背部装配有雷达，格栅造型需隐藏雷达进行美化、且格栅材料不得影响雷达功能。\n"]
[null,"GB 17354-1998《汽车前、后端保护装置》",{"$nulls":8},"d、格栅为黑色，表面带皮纹，皮纹式样以金龙提供样板为准。"]
[null,"GB 20182—2024《商用车驾驶室外部凸出物》",{"$nulls":8},"3、承制厂商需须具备三年以上前保生产经验、有三维数据设计制作能力，根据甲方需求，进行设计和优化。"]
[null,"GB 15741-1995《汽车和挂车号牌板(架)及其位置》",{"$nulls":8},"4、模具应质量良好，成型后产品表面应自然美观有质感，不能采用喷漆工艺掩盖模具的瑕疵；寿命按照≥5000台。"]
[null,"GB/T 9286-1998《色漆和清漆漆膜的划格试验》",{"$nulls":8},"5、检具要求：需配套相应的检具，检验范围为各安装孔及边界尺寸，并提供检具合格三坐标报告、检查基准书，检具数据等文件，检具需要定期检测及出示报告。\n"]
[null,"GB/T 30512-2014《汽车禁用物质要求》",{"$nulls":8},"6、需提供一套RP样件。"]
[null,"GB 11551-2014《汽车正面碰撞的乘员保护》",{"$nulls":8},"7、结构与规格构想\n"]
[{"$nulls":10},"K10前保险杠下部格栅结构，如下所示"]
[{"$nulls":10},"格栅总成尺寸：  长1810mm，宽288mm，高300mm"]
[{"$nulls":10},"格栅通过螺接与卡接方式与上本体固定"]
{"$rows_empty":7}
[null,"主要设计改良及讨论项目",{"$nulls":20},"减轻重量和降低成本管控要点"]
{"$rows_empty":7}
[{"$nulls":22},"品管及生产管控要点"]
[]
[{"$nulls":22},"   1) 零件必须符合造型要求，符合尺寸公差要求；"]
[{"$nulls":22},"   2) 零件无缩痕、无裂纹、无明显熔接痕等缺陷；"]
[{"$nulls":22},"   3) 零件的外观视觉和光洁度必须符合质量检验人员的主观要求；"]
[null,"编 制",null,null,"审 核",null,null,"审 定"]
[]
[]
[]
[]
[null,"　"]